

Software Safety Requirements and Architecture

Lane Assistance

**Document Version: 1.0**

**Template Version 1.0, Released on 2017-06-21**



# Document history

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Editor | Description |
| 1/2/2018 | 1.0 | Joshua Schoenfield | First Submission |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# 

# Table of Contents

[Document history](#_1t3h5sf)

[Table of Contents](#_pyp8fd3vpmy3)

[Purpose](#_c1lz2bx22jid)

[Inputs to the Software Requirements and Architecture Document](#_hjpgfzcjxim1)

[Technical safety requirements](#_lc6owg9q3amb)

[Refined Architecture Diagram from the Technical Safety Concept](#_db3hhee81tpq)


[Software Requirements](#_pul4igmpfvr0)

[Refined Architecture Diagram](#_b7fyegncumoz)

# Purpose

The software requirements and architecture document will outline how the technical safety requirements, requirements for robustness, and requirements to ensure freedom from interference are translated to concrete software safety requirements.

Furthermore, these requirements specify variable names, signal paths and software protocols and mechanisms.



**[Image taken from lesson 19.8]**

# Inputs to the Software Requirements and Architecture Document

## Technical safety requirements

Technical Safety Requirements related to Functional Safety Requirement 01-01 are:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Architecture Allocation** | **Safe State** |
| Technical  Safety  Requirement  01-01 | The LDW safety component shall ensure that the amplitude of the 'LDW\_Torque\_Request' sent to the 'Final electronic power steering Torque' component is below 'Max\_Torque\_Amplitude. | C | 50 ms | LDW Safety Block | LDW torque output is set to zero |
| Technical  Safety  Requirement  01-02 | As soon as the LDW function deactivates the LDW feature, the 'LDW Safety' software block shall send a signal to the car display ECU to turn on a warning light. | C | 50 ms | LDW Safety Block | LDW torque output is set to zero |
| Technical  Safety  Requirement  01-03 | As soon as a failure is detected by the LDW function, it shall deactivate the LDW feature and the 'LDW\_Torque\_Request' shall be set to zero. | C | 50 ms | LDW Safety Block | LDW torque output is set to zero |
| Technical  Safety  Requirement  01-04 | The validity and integrity of the data transmission for 'LDW\_Torque\_Request' signal shall be ensured. | C | 50 ms | Data Transmission Integrity Check | LDW torque output is set to zero |
| Technical  Safety  Requirement  01-05 | Memory test shall be conducted at start up of the EPS ECU to check for any faults in memory. | A | Ignition cycle | Safety Startup: Memory Test Block | LDW torque output is set to zero |

## Refined Architecture Diagram from the Technical Safety Concept

****

# Software Requirements

**Lane Departure Warning (LDW) Amplitude Malfunction Software Requirements:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01 | The LDW safety component shall ensure that the amplitude of the LDW\_Torque\_Request sent to the Final Electronic Power Steering Torque component is below Max\_Torque\_Amplitude | C | 50 ms | LDW Safety Block | LDW torque output is set to zero |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ID | Software Safety Requirement | ASIL | Allocation Software Elements | Safe State |
| Software  Safety  Requirement  01-01-01 | The input signal “Primary\_LDW\_Torq\_Req” shall be read and pre-processed to determine the torque request coming from the “Basic/Main LAFunctionality” SW Component. Signal “processed\_LDW\_Torq\_Req” shall be generated at the end of the processing. | C | LDW\_SAFETY\_INPUT\_PROCESSING | N/A |
| Software Safety Requirement 01-01-02 | In case the “processed\_LDW\_Torq\_Req” signal has a value greater than “Max\_Torque\_Amplitude\_LDW” (maximum allowed safe torque), the torque signal “limited\_LDW\_Torq\_Req” shall be set to 0, else “limited\_LDW\_Torq\_Req” shall take the value of “processed\_LDW\_Torq\_Req”. | C | TORQUE\_LIMITER | “limited\_LDW\_Torq\_Req” = 0 (Nm=Newton-meter) |
| Software Safety Requirement 01-01-03 | The “limited\_LDW\_Torq\_Req” shall be transformed into a signal “LDW\_Torq\_Req” which is suitable to be transmitted outside of the LDW Safety component (“LDW Safety”) to the “Final EPS Torque”component. Also see SofSafReq02-01 and SofSafReq02-02 | C | LDW\_SAFETY\_OUTPUT\_GENERATOR | LDW\_Torq\_Req= 0 (Nm) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-02 | The validity and integrity of the data transmission for LDW\_Torque\_Request signal shall be ensured | C | 50 ms | Data Transmission Integrity Check | N/A |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-02-01 | Any data to be transmitted outside of the LDW Safety component (“LDW Safety”) including "LDW\_Torque\_Req" and “activation\_status” (see SofSafReq03-02) shall be protected by an End2End(E2E) protection mechanism | C | E2ECalc | LDW\_Torq\_Req= 0 (Nm) |
| Software Safety Requirement 01-02-02 | The E2E protection protocol shall contain and attach the control data: alive counter (SQC) and CRC to the data to be transmitted. | C | E2ECalc | LDW\_Torq\_Req= 0 (Nm) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-03 | As soon as a failure is detected by the LDW function, it shall deactivate the LDW feature and the LDW\_Torque\_Request shall be set to zero | C | 50 ms | LDW Safety | LDW torque output is set to zero |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement01-03-01 | Each of the SW elements shall output a signal to indicate any error which is detected by the element. Error signal = error\_status\_input(LDW\_SAFETY\_INPUT\_PROCESSING), error\_status\_torque\_limiter(TORQUE\_LIMITER), error\_status\_output\_gen(LDW\_SAFETY\_OUTPUT\_GENERATOR) | C | All | N/A |
| Software Safety Requirement01-03-02 | A software element shall evaluate the error status of all the other software elements and in case any 1 of them indicates an error, it shall deactivate the LDW feature (“activation\_status”=0) | C | LDW\_SAFETY\_ACTIVATION | Activation\_status = 0 (LDW function deactivated) |
| Software Safety Requirement01-03-03 | In case of no errors from the software elements, the status of the LDW feature shall be set to activated (“activation\_status”=1) | C | LDW\_SAFETY\_ACTIVATION | N/A |
| Software Safety Requirement01-03-04 | In case an error is detected by any of the software elements, it shall set the value of its corresponding torque to 0 so that “LDW\_Torq\_Req” is set to 0 | C | All | LDW\_Torq\_Req = 0 |
| Software Safety Requirement01-03-05 | Once the LDW functionality has been deactivated, it shall stay deactivated till the time the ignition is switched from off to on again. | C | LDW\_SAFETY\_ACTIVATION | Activation\_status = 0 (LDW function deactivated) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-04 | As soon as the LDW function deactivates the LDW feature, the LDW Safety software block shall send a signal to the car display ECU to turn on a warning light | C | 50 ms | LDW Safety | LDW torque output is set to zero |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-04-01 | When the LDW function is deactivated (activation\_status set to 0), the activation\_status shall be sent to the car displayECU. | C | LDW\_SAFETY\_ACTIVATION, CarDisplay ECU | N/A |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-05 | Memory test shall be conducted at start up of the EPS ECU to check for any faults in memory | A | Ignition Cycle | Memory Test | LDW torque output is set to zero |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-05-01 | A CRC verification check over the software code in the Flash memory shall be done every time the ignition is switched from off to on to check for any corruption of content. | A | MEMORYTEST | Activation\_status = 0 |
| Software Safety Requirement 01-05-02 | Standard RAM tests to check the data bus, address bus and device integrity shall be done every time the ignition is switched from off to on (E.g.walking 1s test, RAM pattern test. Refer RAM and processor vendor recommendations ) | A | MEMORYTEST | Activation\_status = 0 |
| Software Safety Requirement 01-05-03 | The test result of the RAM or Flash memory shall be indicated to the LDW\_Safety component via the “test\_status” signal | A | MEMORYTEST | Activation\_status = 0 |
| Software Safety Requirement 01-05-04 | In case any fault is indicated via the “test\_status” signal the INPUT\_LDW\_PROCESSING shall set an error on error\_status\_input (=1) so that the LDW functionality is deactivated and the LDWTorque is set to 0 | A | LDW\_SAFETY\_INPUT\_PROCESSING | Activation\_status = 0 |

# 

# Refined Architecture Diagram

The refined system architecture, incorporating the ASIL labels of each component can be found in the diagram below:

****